F

MAC Pos as found in DEBUG: 24.16ft
LEMAC Pos as found in DEBUG: -7.71ft

Empty weight
	Arm: -13.3ft
	Weight: 112748kg
	Moment: Arm * Weight = -1499548.4 kg*ft

77kg in Pilot station
	Arm: 82ft
	Weight: 77kg
	Moment: Arm * Weight = 6314 kg*ft
77kg in FO station
	Arm: 82ft
	Weight: 77kg
	Moment: Arm * Weight = 6314 kg*ft
77kg in FE station
	Arm: 80ft
	Weight: 77kg
	Moment: Arm * Weight = 6160 kg*ft

Total:
	Weight: Sum = 112979kg
	Moment: Sum = -1480760.4 kg*ft
	CG: Moment / Weight = -13.11ft (-13.1065065189)

As %MAC
	abs(((CG - LEMAC) / MAC) * 100)
	abs(((-13.11 - -7.71) / 24.16) * 100)
	22.35

PAX

MAC Pos as found in DEBUG: 24.16ft
LEMAC Pos as found in DEBUG: -7.71ft

Empty weight
	Arm: -13.3ft
	Weight: 128809kg
	Moment: Arm * Weight = -1713159.7 kg*ft

77kg in Pilot station
	Arm: 82ft
	Weight: 77kg
	Moment: Arm * Weight = 6314 kg*ft
77kg in FO station
	Arm: 82ft
	Weight: 77kg
	Moment: Arm * Weight = 6314 kg*ft
77kg in FE station
	Arm: 80ft
	Weight: 77kg
	Moment: Arm * Weight = 6160 kg*ft

Total:
	Weight: Sum = 129040kg
	Moment: Sum = -1694371.7 kg*ft
	CG: Moment / Weight = -13.13ft (-13.1305928394)

As %MAC
	abs(((CG - LEMAC) / MAC) * 100)
	abs(((-13.13 - -7.71) / 24.16) * 100)
	22.35